#### DISARMING

##### All Models

NOTE: All SRS electrical wiring harnesses and connectors are covered with YELLOW outer insulation. Do not use electrical test equipment on any circuit related to the SRS (air bag) sensors. When installing SRS components, always install with the arrow marks facing the front of the vehicle.

To disarm the SRS system turn the ignition switch toOFF position. Then disconnect the both battery cables starting with the negative cable first and wait at least 10 minutes after the cables are disconnected. Be sure to insulate the battery terminal ends.

##### Arming

To arm the SRS system turn the ignition switch to OFF position. Connect the both battery cables starting with the positive cable first.

NOTE: The SRS or air bag system is equipped with a self-diagnostic operation. After turning the ignition key to the ON or START position, the AIR BAG warning lamp will illuminate for 7 seconds. After 7 seconds, the AIR BAG lamp will extinguish if no malfunction is detected. If the AIR BAG lamp does not extinguish after 7 seconds, check the SRS self diagnostic system for a malfunction.