#### REMOVAL & INSTALLATION

##### EGR Control Valve

1. Remove the nuts which attach the EGR tube and/or the BP tube to the EGR valve (if so equipped).
2. Unscrew the mounting bolts and remove the heat shield plate from the EGR control valve (if so equipped).
3. Tag and disconnect the EGR vacuum hose(s).
4. Unscrew the mounting bolts and remove the EGR control valve.

   To install:

5. Install the EGR valve assembly with mounting bolts (torque retaining bolts EVENLY) to intake manifold location.
6. Connect all vacuum hoses and install the heat shield if so equipped.
7. Connect EGR tube or BP tube to the EGR valve if so equipped. If replacing the EGR valve assembly always be sure that the new valve is identical to the old one.