### Washer Fluid Reservoir

#### REMOVAL & INSTALLATION

##### Front and Rear

1. Disconnect the negative battery cable and reservoir electrical connector.
2. Disconnect the fluid tube from the washer motor. If the tube is too tight to remove, do not force. Heat the tube with a heat gun if the tube has no extra slack or cut the tube at the motor end.
3. Remove the reservoir retaining bolts and slide out of the bracket.
4. Installation is the reverse of removal. Apply petroleum jelly to the motor nipple before installing the washer tube.

   NOTE: A check valve is installed in the washer fluid line. Be careful not to connect check valve to washer tube in the wrong direction.