#### LEVEL CHECK

Check the level of the lubricant in the steering gear every 15,000 miles or 12 months. If the level is low, check for leakage. Any oily film is not considered a leak; solid grease must be present. The lubricant is added and checked through the filler plug hole in the top of the steering gearbox.

Fig. 1: Check the fluid level in the steering gearbox through the filler hole in top