#### REMOVAL & INSTALLATION

NOTE: Models built in 1985 and later years do not use a separate proportioning valve.

1. Disconnect and plug the brake lines at the valve.
2. Unscrew the mounting bolt(s) and remove the valve.

   NOTE: Do not disassemble the valve.

3. Installation is in the reverse order of removal. Bleed the complete brake system.

   Fig. 1: Proportioning valve — Stanza

   Fig. 2: Cross-section of proportioning valve — most models similar

   Fig. 3: Bleeding the brakes