#### SOLENOID REPLACEMENT

NOTE: The starter solenoid is also know as the magnetic switch assembly.

1. Remove the starter from the engine as outlined above.
2. Place the starter in a vise or equivalent to hold the starter in place while you are working on the solenoid. DO NOT tighten the vise to tight around the case of the starter. The case will crack if you tighten the vise too much.
3. Loosen the lock-nut and remove the connection from the starter motor going to the M terminal of the solenoid or bottom terminal of the solenoid.
4. Remove the securing screws and remove the solenoid.
5. Install the solenoid to the starter and tighten the securing screws.
6. Install the connection and lock-nut at bottom terminal of the starter.