#### ADJUSTMENT

NOTE: No adjustment is necessary on Stanza Wagon 4WD, 240SX and 1990–92 Stanza (one-piece bearing hub assembly).

NOTE: Make sure all parts are cleaned, apply multi-purpose grease sparingly to rubbing surface of the spindle, between surface of lock washer and outer wheel bearing, grease seal and dust cap in the proper areas.

1. Raise the rear of the vehicle and support it on jackstands.
2. Remove the wheel.
3. Remove the bearing dust cap with a pair of channel locks pliers or equivalent.
4. Remove the cotter pin and retaining nut cap, dispose of the cotter pin.
5. On 1982–86 Stanza models — tighten the wheel bearing lock-nut 29–33 ft. lbs.

   NOTE: On 1987–89 Stanza and Stanza Wagon 2WD — tighten the wheel bearing lock-nut 18–25 ft. lbs.

6. Rotate the drum back and forth a few revolutions to seat wheel bearing.

   NOTE: On 1987–89 Stanza and Stanza Wagon 2WD — loosen wheel bearing lock-nut so that the preload becomes 0 then torque to 6.5–8.7 ft. lbs. turn wheel hub several times in both directions and retorque to 6.5–8.7 ft. lbs.

7. On 1982–86 Stanza only, after turning the wheel, recheck the torque (29–33 ft. lbs. is specification for these vehicles) of the nut, then loosen it 90°from its position.
8. Install the retaining nut cap. Align the cotter pin holes in the nut cap with hole in the spindle by tighten the nut no more than 15°to align the holes.
9. Install the NEW cotter pin, bend up its ends and install the dust cap.