### Outside Mirrors

#### REMOVAL & INSTALLATION

##### Manual Type

1. Remove control knob handle.
2. Remove door corner finisher panel.
3. Remove mirror body attaching screws, and then remove mirror body
4. Installation is in the reverse order of removal.

   NOTE: Apply sealer to the rear surface of door corner finisher panel during installation to prevent water leak.

   Fig. 1: Two types of door corner finisher panels

   Fig. 2: Removing mirror mounting screws

   Fig. 3: Apply sealer to rear surface of finisher panel

##### Power Type

1. Remove door corner finisher panel.
2. Remove mirror body attaching screws, and then remove mirror body
3. Disconnect the electrical connection.

   NOTE: It may be necessary to remove the door trim panel to gain access to the electrical connection.

4. Installation is in the reverse order of removal.

   Fig. 4: Power mirror installation