#### REMOVAL & INSTALLATION

1. Remove the air cleaner.
2. Disconnect and mark the electrical connector(s), the fuel and the vacuum hoses from the carburetor.
3. Remove the throttle lever.
4. Remove the four nuts and washers retaining the carburetor to the manifold.
5. Lift the carburetor from the manifold. Do not tilt the carburetor over when removed from the manifold.

   To install:

6. Remove and discard the gasket used between the carburetor and the manifold. Clean all vacuum passages on intake manifold if necessary.
7. Install carburetor on the manifold, use a new base gasket and torque the carburetor mounting nuts EVENLY to 9–13 ft. lbs.
8. Install the throttle lever.
9. Connect the electrical connector(s), the fuel and the vacuum hoses to the carburetor. Replace the fuel line gas clamps as necessary.
10. Install the air cleaner.
11. Start engine, warm engine and adjust as necessary.