#### MASTER CYLINDER BLEEDING

1. Place the master cylinder in a vise.
2. Connect two lines to the fluid outlet orifices, and into the reservoir.
3. Fill the reservoir with brake fluid.

   Fig. 1: Master cylinder and brake booster — 1992 240SX shown

   Fig. 2: Bench bleeding the master cylinder

4. Using a wooden dowel, depress the pushrod slowly, allowing the pistons to return. Do this several times until the air bubbles are all expelled.
5. Remove the bleeding tubes from the master cylinder, plug the outlets and install the caps.