### Side Oil Seal

#### REMOVAL & INSTALLATION

Fig. 1: Removing side oil seal

Fig. 2: Installing side oil seal

Fig. 3: Checking the final drive unit fluid level

1. Remove the halfshaft––refer to the necessary service procedures.
2. Remove side flange if so equipped (matchmark for correct installation) using suitable puller.
3. Remove the oil seal.

   To install:

4. Apply multi-purpose grease to sealing lips of oil seal. Press oil seal into carrier.
5. Install side flange if so equipped with special tool J39352 or equivalent.
6. Install the halfshaft. Check fluid level.