### Rocker Arm Cover

#### REMOVAL & INSTALLATION

1. Disconnect the negative battery cable. Remove or disconnect any electrical lines, hoses or tubes which may interfere with the removal procedures.

   NOTE: It may be necessary to remove the air cleaner (carburetor models) or the air duct (EFI and turbo models).

2. Remove the rocker arm cover-to-cylinder head mounting screws , then lift the cover from the cylinder head.
3. Using a scraper or equivalent, clean the gasket mounting surfaces.
4. To install, use a NEW gasket and/or RTV sealant, then position the rocker arm cover in place. Torque the cover bolts-to-cylinder head EVENLY (working from the center to the end of the cover) to 5–8 ft. lbs. on Z series engine, 2–4 ft. lbs. on C and V series engines and 5–7 ft. lbs. on K series engines.

   NOTE: When using RTV sealant apply a even bead and make sure the surface that you are working on is very clean before applying sealer.