#### REMOVAL & INSTALLATION

On all models, the coil assembly is either mounted to the wall of the engine compartment or the engine. To remove disconnect and mark all electrical connections — remove the coil assembly, then transfer coil mounting bracket if so equipped to the new coil. When installing the new coil make sure that the coil wire and all other electrical connections are properly installed.