### Fuel Pressure Regulator

#### REMOVAL & INSTALLATION

1. Relieve fuel pressure from system. Disconnect the negative battery cable.
2. Disengage vacuum tube connecting regulator to intake manifold from pressure regulator.
3. Remove screws securing pressure regulator.
4. Unfasten hose clamps, and disconnect pressure regulator from fuel hose.

   NOTE: Place a rag under fuel pipe to absorb any remaining fuel.

5. To install, reverse the removal procedure.