### Brake Drums

#### REMOVAL & INSTALLATION

##### 200SX and 1990–92 Stanza Models

1. Raises the rear of the vehicle and support it on jack stands.
2. Remove the wheels.
3. Release the parking brake.
4. Pull off the brake drums. On some models there are two threaded service holes in each brake drum. If the drum will not come off, fit two correct size bolts in the service holes and screw them in: this will force the drum away from the axle.
5. If the drum cannot be easily removed, back off the brake adjustment.

   NOTE: Never depress the brake pedal while the brake drum is removed.

6. Installation is the reverse of removal procedure.

   Fig. 1: Brake drum removal

   Fig. 2: Brake drum and bearing removal

##### 1982–89 Stanza and Stanza Wagon Models

NOTE: For rear wheel bearing service procedures refer to Section 8.

1. Raise the rear of the vehicle and support it on jackstands.
2. Remove the wheels.
3. Release the parking brake.
4. Remove the grease cap, the cotter pin and the adjusting cap and the wheel bearing nut.
5. Pull off the drum, taking care not to drop the tapered bearing assembly.
6. Install the drum assembly to the vehicle. Adjust the wheel bearing — refer to the necessary service procedures.
7. Install the wheels.