### ASCD Cable

#### REMOVAL & INSTALLATION

1. Disconnect the cable from the actuator assembly — loosen the locknut at actuator assembly and remove the rubber boots.
2. Loosen the locknut at intake manifold bracket. Remove the cable.
3. Installation is the reverse of the removal procedures. Adjust the cable as required. When removing or installing wire end use care not damage. Check system for proper operation.