#### LEVEL CHECK

Check the coolant level every 3,000 miles or once a month. In hot weather operation, it may be a good idea to check the level once a week. Check for loose connections and signs of deterioration of the coolant hoses. Maintain the coolant level 3⁄4 –1 1⁄4 in. (19–32mm) below the level of the filler neck when the engine is cold.

Check the coolant level in the coolant recovery bottle when the engine is cold; the level should be up to the MAX mark. If the bottle is empty, check the level in the radiator and refill as necessary, then fill the bottle up to the MAX level.

CAUTION
Never remove the radiator cap when the vehicle is hot or overheated. Wait until it has cooled. Place a thick cloth over the radiator cap to shield yourself from the heat and turn the radiator cap, SLIGHTLY, until the sound of escaping pressure can be heard. DO NOT turn any more; allow the pressure to release gradually. When no more pressure can be heard escaping, remove the cap with the heavy cloth, CAUTIOUSLY.

NOTE: Never add cold water to an overheated engine while the engine is not running.

After filling the radiator, run the engine until it reaches normal operating temperature, to make sure that the thermostat has opened and all the air is bled from the system.

Fig. 1: If the engine is HOT, cover the radiator cap with a rag

Fig. 2: Some type radiator caps have pressure release levers

Fig. 3: Checking coolant level in radiator

Fig. 4: Checking coolant level in recovery bottle

Fig. 5: Always check the gasket in the radiator cap when checking coolant level