### Speedometer Cable

#### REMOVAL & INSTALLATION

##### All Models

NOTE: The speedometer cable connector-to instrument cluster/combination meter has a snap release––simply press on the connector tab to release it.

1. Loosen the lock nut at the rear extension housing on transmission/transaxle assembly.

   Fig. 1: Removing the speedometer cable

   Fig. 2: Slide the speedometer cable out from the vehicle

   Fig. 3: Installing the speedometer cable

2. Disconnect the negative battery cable. Remove the instrument cluster/ combination meter––refer to the necessary service procedure.
3. Slide the speedometer cable up to free it.
4. Detach the speedometer cable from all retaining (4) points.
5. Remove the grommet from the upper dash panel by hand.
6. Pull out the speedometer cable from the vehicle.
7. Installation is the reverse of the removal procedure. Make sure that the speedometer cable assembly is properly lubricated. Install the cable end and hollow portion in the transmission/transaxle rear extension in the correct manner. Torque the lock nut to 7–11 ft. lbs.