#### CHECKING CAMSHAFT END-PLAY

After the camshaft has been installed, end-play should be checked. The camshaft sprocket should not be installed on the cam. Use a dial gauge to check the end-play, by moving the camshaft forward and backward in the cylinder head. End-play specifications for the CA20E, CA18ET, Z20/22 series and KA24E engines should not exceed 0.20mm. On the VG30E engine the camshaft end-play should be between 0.03–0.06mm.