#### REPAIRING DAMAGED THREADS

Fig. 1: Damaged bolt hole threads can be replaced with thread repair inserts

Fig. 2: Standard thread repair insert (left), and spark plug thread insert

Fig. 3: Drill out the damaged threads with the specified size bit. Be sure to drill completely through the hole or to the bottom of a blind hole

Fig. 4: Using the kit, tap the hole in order to receive the thread insert. Keep the tap well oiled and back it out frequently to avoid clogging the threads

Fig. 5: Screw the insert onto the installer tool until the tang engages the slot. Thread the insert into the hole until it is 1⁄4 – 1⁄2 turn below the top surface, then remove the tool and break off the tang using a punch

Several methods of repairing damaged threads are available. Heli-Coil(r) (shown here), Keenserts(r) and Microdot(r) are among the most widely used. All involve basically the same principle — drilling out stripped threads, tapping the hole and installing a prewound insert — making welding, plugging and oversize fasteners unnecessary.

Two types of thread repair inserts are usually supplied: a standard type for most inch coarse, inch fine, metric course and metric fine thread sizes and a spark lug type to fit most spark plug port sizes. Consult the individual tool manufacturer's catalog to determine exact applications. Typical thread repair kits will contain a selection of prewound threaded inserts, a tap (corresponding to the outside diameter threads of the insert) and an installation tool. Spark plug inserts usually differ because they require a tap equipped with pilot threads and a combined reamer/tap section. Most manufacturers also supply blister-packed thread repair inserts separately in addition to a master kit containing a variety of taps and inserts plus installation tools.

Before attempting to repair a threaded hole, remove any snapped, broken or damaged bolts or studs. Penetrating oil can be used to free frozen threads. The offending item can usually be removed with locking pliers or using a screw/stud extractor. After the hole is clear, the thread can be repaired as shown in the kit manufacturer's instructions.