### Upper Control Arms

#### REMOVAL AND INSTALLATION

##### 300ZX

Fig. 1:Upper control arm identification marks — 300ZX

1. Raise and properly support vehicle.
2. Remove appropriate wheel assembly.
3. Support the lower control arm using a separate jack.
4. Remove the two mounting bolts connecting the upper control arm and remove the assembly.

   To install

5. Install the control arm (link), with theA identification mark toward the axle side and facing upward. Lightly tighten the mounting bolts.
6. Install wheel and lower vehicle.
7. With full weight of vehicle on the ground, torque the mounting bolts to 65–80 ft. lbs. (88–108 Nm).