#### REMOVAL & INSTALLATION

1. Disconnect the negative battery terminal.
2. Disconnect the two lead wires and connector from the alternator.
3. Loosen the drive belt adjusting bolt and remove the belt.
4. Unscrew the alternator attaching bolts and remove the alternator from the vehicle.

   To install:

5. Mount the alternator to the engine and partially tighten the attaching bolts.
6. Reconnect the lead wires and connector to the alternator.
7. Install the alternator drive belt.
8. Adjust the alternator belt correctly and completely tighten the mounting bolts.

   NOTE: The correct belt tension is about 1⁄4 – 1⁄2 in. (613mm) play on the longest span of the drive belt. The alternator belt tension is quite critical. A belt that is too tight may cause alternator bearing failure; one that is too loose will cause a gradual battery discharge.

9. Connnect the battery cable. Start the engine and check for proper operation.