### Signal and Marker Lights

#### REMOVAL & INSTALLATION

##### Front Turn Signal and Parking Lights

1. Refer to the illustrations. Remove turn signal/parking light lens with retaining screws.
2. Slightly depress the bulb and turn it counterclockwise to release it.
3. To install the bulb carefully push down and turn bulb clockwise at the same time.
4. Install the turn signal/parking light lens with retaining screws.

   Fig. 1: Light bulb removal and installation — 240SX

   Fig. 2: Light bulb removal and installation — 240SX

   Fig. 3: Light bulb removal and installation — 240SX

   Fig. 4: Light bulb removal and installation — 240SX

##### Side Marker Lights

1. Refer to the illustrations. Remove side marker light lens with retaining screws.
2. Turn the bulb socket counterclockwise to release it from lens.
3. Pull bulb straight out.
4. To install the bulb, carefully push it straight in.
5. Turn the bulb socket clockwise to install it in the lens.
6. Install side marker light lens with retaining screws.

   Fig. 5: Light bulb removal and installation — Stanza

   Fig. 6: Light bulb removal and installation — Stanza

   Fig. 7: Light bulb removal and installation — Stanza

   Fig. 8: Light bulb removal and installation — Stanza

##### Rear Turn Signal, Brake and Parking Lights

1. Refer to the illustrations. Remove rear trim panel in rear of vehicle if necessary to gain access to the bulb socket.
2. Slightly depress the bulb and turn it counterclockwise to release it.
3. To install the bulb, carefully push down and turn bulb clockwise at the same time.
4. Install trim panel if necessary.

   Fig. 9: Light bulb removal and installation — 200SX

   Fig. 10: Light bulb removal and installation — 200SX

   Fig. 11: Light bulb removal and installation — 200SX

##### High-Mount Brake Light/Dome Light/Cargo Light/License Plate Light

1. Unfasten any necessary retainers, then remove the lens to access the bulb socket.
2. Identify the type of bulb and remove it using the appropriate technique. Refer to the illustrations.
3. Install the bulb carefully, by reversing the removal steps.
4. Install the lens.

   Fig. 12: Common Light Bulb Chart

   TROUBLESHOOTING BASIC LIGHTING PROBLEMS