### Brake Drums

#### REMOVAL AND INSTALLATION

##### Altima, Maxima, Sentra and 200SX

CAUTION
Brake shoes may contain asbestos, which has been determined to be a cancer causing agent. Never clean the brake surfaces with compressed air! Avoid inhaling any dust from any brake surface! When cleaning brake surfaces, use a commercially available brake cleaning fluid.

1. Raise the rear of the vehicle and support it on jackstands.
2. Remove the wheels.
3. Release the parking brake.
4. Remove the brake drum from the brake shoes. Using two 8mm x 1.25 bolts, tighten the bolts evenly to remove the drum.
5. If necessary, back off the brakes to remove the drum.

   To install:

6. Install the drum assembly to the vehicle.
7. Install the wheels.
8. Adjust the rear brakes.