#### CHECKING CAMSHAFT LOBE HEIGHT

Use a micrometer to check cam (lobe) height, making sure the anvil and the spindle of the micrometer are positioned directly on the heel and tip of the cam lobe as shown in the accompanying illustration. Use the specifications in the following chart to determine the lobe wear.

Fig. 1: Use a micrometer to check camshaft cam lobe height

Fig. 2: Camshaft specifications