### Instrument Pad Assembly

#### REMOVAL & INSTALLATION

To remove the instrument pad assembly — refer to the Exploded Views of "Instrument Pad Assembly''. When removing instrument pad assembly, remove the defroster grille, combination meter, A/C or heater control, and all necessary trim panels. These parts are mostly plastic, so do not use excessive force and be careful not to damage them.

On 240SX models, when removing the Head-Up Display (HUD) finisher, be careful not to scratch the HUD's reflective surface. To prevent this, cover the finisher and reflective surface with a protective covering.

Fig. 1: Instrument panel/pad assembly 1983 200SX

Fig. 2: Instrument panel/pad assembly 1984–88 200SX

Fig. 3: Instrument panel/pad assembly 1990–92 240SX (part 1)

Fig. 4: Instrument panel/pad assembly 1990–92 240SX (part 2)

Fig. 5: Instrument panel/pad assembly 1983 Stanza

Fig. 6: Instrument panel/pad assembly 1987 Stanza

Fig. 7: Instrument panel/pad assembly 1990–92 Stanza (part 1)

Fig. 8: Instrument panel/pad assembly 1990–92 Stanza (part 2)