### Seats

#### REMOVAL & INSTALLATION

##### Front Assembly

NOTE: On power seat models remove the seat then remove the power seat motor assembly and drive cable. Refer to the exploded view of Front Seat Assembly.

1. Remove front seat mounting bolts.
2. Remove front seat assembly.
3. Installation is in the reverse order of removal.

   Fig. 1: Front seat assembly — 1988 200SX

   Fig. 2: Front seat assembly — 240SX

   Fig. 3: Front seat assembly — 1992 Stanza

##### Rear Assembly

1. Remove rear seat cushion mounting bolts.
2. Remove screw attaching luggage floor carpet.
3. Remove rear seat back by tilting forward and pulling straight up.

   NOTE: On hatchback models the rear seat back is remove similar as above.

   Fig. 4: Rear seat assembly — 1988 200SX

   Fig. 5: Rear seat assembly — 240SX

   Fig. 6: Rear seat assembly — 1992 Stanza