#### OXIDES OF SULFUR

Oxides of sulfur (SOx) were initially ignored in the exhaust system emissions, since the sulfur content of gasoline as a fuel is less than 1⁄10 of 1 percent. Because of this small amount, it was felt that it contributed very little to the overall pollution problem. However, because of the difficulty in solving the sulfur emissions in industrial pollution and the introduction of catalytic converters to automobile exhaust systems, a change was mandated. The automobile exhaust system, when equipped with a catalytic converter, changes the sulfur dioxide (SO2) into sulfur trioxide (SO3).

When this combines with water vapors (H2O), a sulfuric acid mist (H2SO4) is formed and is a very difficult pollutant to handle since it is extremely corrosive. This sulfuric acid mist that is formed, is the same mist that rises from the vents of an automobile battery when an active chemical reaction takes place within the battery cells.

When a large concentration of vehicles equipped with catalytic converters are operating in an area, this acid mist may rise and be distributed over a large ground area causing land, plant, crop, paint and building damage.