### Brake Disc (Rotor)

#### REMOVAL & INSTALLATION

##### 200SX and 240SX Models — Rear Wheel Drive

1. Raise and support the front of the vehicle safely and remove the wheels.
2. Remove the brake caliper assembly and wheel hub/bearing assembly, if necessary. Refer to the necessary procedures in Section 8. Make sure not to twist the brake hose.
3. Remove the brake disc/wheel hub from the vehicle.
4. Installation is the reverse of removal. Adjust the wheel bearings if necessary.