# SPECIFICATIONS AND MAINTENANCE INTERVALS

## 200SX, 240SX, 300ZX, Altima, Maxima, NX, Pulsar, Sentra, Stanza

Fig. 1: 1.6L GA16DE Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 2: 2.0L SR20DE Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 3: 2.4L KA24DE Altima Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 4: 2.4L KA24DE 240SX Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 5: 3.0L VG30DE Engine Firing order: 1–2–3–4–5–6 Distributorless ignition system one coil on each cylinder

Fig. 6: Lower intake manifold torque sequence — 1.6L engines

Fig. 7: Upper intake manifold torque sequence — 1.6L engines

Fig. 8: Intake manifold torque sequence — 1993–95 Sentra models with 2.0L (SR20DE) engines

Fig. 9: Intake manifold torque sequence — 2.4L engines

Fig. 10: Intake manifold torque sequence — 3.0L (VG30DE and VG30DETT) engines

Fig. 11: Cylinder head torque sequence — 1.6L GA16i, GA16DE engine

Fig. 12: Cylinder head torque sequence — 2.0L SR20DE engines

Fig. 13: Cylinder head torque sequence — 2.4L KA24DE engines

Fig. 14: Right cylinder head torque sequence — 3.0L VG30DE and VG30DETT engines

Fig. 15: Left cylinder head torque sequence — 3.0L VG30DE and VG30DETT engines

Fig. 16: 1.6L GA16DE Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 17: 2.0L SR20DE Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 18: 2.4L KA24DE Altima Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 19: 2.4L KA24DE 240SX Engine Firing order: 1–3–4–2 Distributor rotation: Counterclockwise

Fig. 20: 3.0L VG30DE and 3.0L VQ30DE Engines Firing order: 1–2–3–4–5–6 Distributorless ignition system one coil on each cylinder

Fig. 21: Lower intake manifold torque sequence — 1.6L engines

Fig. 22: Upper intake manifold torque sequence — 1.6L engines

Fig. 23: Lower intake manifold torque sequence — 200SX with 2.0L engines

Fig. 24: Upper intake manifold torque sequence — 200SX with 2.0L engines

Fig. 25: Intake manifold torque sequence — 2.4L engines

Fig. 26: Intake manifold torque sequence — 3.0L (VG30DE and VG30DETT) engines

Fig. 27: Intake manifold torque sequence — 3.0L (VQ30DE) engine

Fig. 28: Cylinder head torque sequence — 1.6L GA16i, GA16DE engine

Fig. 29: Cylinder head torque sequence — 2.0L SR20DE engines

Fig. 30: Cylinder head torque sequence — 2.4L KA24DE engines

Fig. 31: Right cylinder head torque sequence — 3.0L VG30DE and VG30DETT engines

Fig. 32: Left cylinder head torque sequence — 3.0L VG30DE and VG30DETT engines

Fig. 33: Right cylinder head torque sequence — 3.0L VQ30DE engine

Fig. 34: Left cylinder head torque sequence — 3.0L VQ30DE engine